Single Glazing' Glass

Advantages

1-Excellent light transmittance, magnificent optical performance and stable chemical properties.

2-Flat and smooth surface, no visible defect.

3-Easy to be cut, bent, insulated, tempered, coated and laminated.

Features

1 -We can also cut size and deal with customer required sized, also edge polishing.

2 -Features: Smooth surface , even thickness, high transmittance ,no wave, no scratch, no bubble,

thickness tolerance reach the national standards.

3 -Function and application: can be applied in the fields of building decorations, mirror making, laminated,

tempered, optical instruments.

Applications

Float glass is usually regarded as raw material, which is processed to laminated glass, tempered glass,

insulated glass, silk screen printing glass, etc. Clear f10at glass is widely used in buildings, hotels, doors,

windows, etc.

-Facades and curtai walls -External walls of revolving doors and exposed elevators -Stairs, handrails, skylights -partitions, display shelves and furniture

Quality Standards

CE(BS EN 572), CE, Iran ISIRI standard,ISO.